Travel buddy LED light fitting guide,

Remove top and bottom rivets on front panel by drilling them out Don’t go to deep

Ease back outer shell pushing it back 40mm, sometimes cord grip may need to be unlocked by anticlockwise turn and use screwdriver to flip open,

To remove LED light using long nose pliers grip white section of LED and twist slightly and pull this should leave red cover still attached to front panel, it may be best to snip wires close to light and connect using crimp joiners provided, much easier than trying to connect to original element wires

I have included some insulation to wrap/place around LED,

If you need help you can call us on 03-54413388

Kind regards Darren

Travel Buddy Ovens